

**JANUARY 2022 MAINTENANCE Updates**

**Tractors and mowers**

|  |  |
| --- | --- |
| **EquipmentUsed** | **Ditches Mowed** |
| ZTRs | 107, 110, 115, 122, 308, 100-A, 100-C, 100-D, 100-D2, 110-B, 110-C, 122-A, DD6 Complex |
| Tractors | 102, 300, 307, 308, 309, 400, 406, 502, 551, 570, 600, 601, 603, 803, 100-D, 123-D, 308-A, 309-A, 406-B, 502-E, 551-B2A, 551-B3A, 551-B3D, 551-B3E, 551-C, 551-D, 551-E, 551-F, 552-C, 601-A, 601-B, 601-C, 601-D, 601-E, 602-A, 602-B, 603-C, 603-E1, 616-A, 8002-B1, 802-B, 802-D, 803-A, 814-A, DD6 Complex, Pond A, WCDP |

**Long-Stick and Marsh Master Mowing**

|  |  |  |
| --- | --- | --- |
| **Ditch** | **Location** | **Description of Work Performed** |
| Gulf Terrace Detention Basin | Phelan Blvd. | Marsh Master® Mowing – 215 feet |
| 603-E2 | Lawhon Rd. | Long-stick Mowing - 5,200 feet |
| 603-E1 | Lawhon Rd. | Long-stick Mowing – 1,300 feet |

**Herbicide Spraying**

|  |
| --- |
| **Ditches Sprayed** |
| N/A |

**Long-Stick Slashing**

|  |  |  |
| --- | --- | --- |
| **Ditch** | **Location** | **Description of Work Performed** |
| 202-B | Wescalder | Slashed trees/brush  |
| 1000-A | Keith Rd. | Slashed 1,700 feet on North side of ditchSlashed 1,700 feet on South side of ditch |

**Completed Maintenance Work**

| **Ditch** | **Location** | **Description of Work Performed** |
| --- | --- | --- |
| 100  | Savannah Trace | Washout repair |
| 119 | Edson Dr. | Re-set gate and fence post |
| 202-B | Wescalder | Cleaned 4,600 feet of ditch |
| 202-E1C | Pheland Blvd. | Reset corner post and gate |
| 400 | Boyt Rd. | Constructed 20-ft wire gap |
| 511-B | Cole Dr. | Installed 2/36-in x 30-ft HDPE pipe |
| 608 | S. China Rd. | Cleaned 22,000 feet of ditch |
| 702 | Mesa Ln. | Removed old pipe |
| 803 | McDermand Rd. | Constructed 20-ft wire gap |
| 804-E | McDermand Rd. | Cleaned 3,200 feet of ditch |
| 1000-A | Keith Rd. | Set 4/24-in x 40-ft downspoutsSet 36-in x 40-ft HDPE crossing |
| 1205 | Gentry Rd. | Set 18-in x 30-ft HDPE pipe |
| 1205-A | Reins Rd. | Constructed 30-ft swing gate |
| 8201 | GIWW – Structure #1 | Installed 4 wooden flap gates |
| 8202-B | Labelle Rd. | Repaired 3 washouts |
| 8202-B | Labelle Rd. | Repaired washout |